**3.1 Mount Backboard**

Purchase a 2’ x 2’ backboard (smooth 3/4“ plywood or white melamine) secure the white telecom backboard to wall using appropriate mounting hardware. The specific mounting location of the backboard will be determined by CEG during the check-in process.

As a general rule, the top of the backboard should be mounted 6’ 6”from the floor and with the 2’ section of the backboard mounted horizontally. Use four 2”molly screws, attach 2” in from each corner of the backboard.

* Do not attach the backboard where its presence will cause interference with existing infrastructure (doors, cabinetry, electrical, plumbing, etc.). Check for hidden plumbing or electrical wiring before drilling through wall.