**3.9 Wire and Cable Management between buildings**

Connect the two buildings using conduit. Please run two CAT6 cables in the pipe. Terminate and label all cables connecting the two buildings, you do not need to connect both cables to the LAN. The second is a backup cable.

Fasten the conduit to the wall and fence.