**3.2 Install Equipment**

The network equipment is to be mounted to the backboard securely using screws mounted to the holes in the back of the equipment. If the equipment cannot be mounted using screws, use a strap that will allow access to cabling and the monitoring lights (if applicable).

Network equipment should be mounted on the left side of the backboard from the top of the backboard in the following sequence (see Attachment 2 for additional information):

1. Patch panel
2. Switches
3. Routers
4. Modem